*K.LOKESH*

*INTERIOR & EXTERIOR PAINTING DECORATORS*

#681, MAIN, 2nd CROSS, MATHIKERE, BENGALURU-560054

MOBILE: 9964231473, 9738438045

Email us @: lokeshdeeksha55@gmail.com

Quotation for Repaint

(With Material and Labour)

* OUTSIDE:

1. Building Washing:

* Washing full building with pressure water jet
* Lumpsum Amount (Rs. 15,000)

1. Crack Filling:

* Crack cutting from machine ½ to 1mm
* Filling Asian crack seal 2times
* Lumpsum Amount (Rs. 30,000)

1. Dam Proof:

* 1 Coat Asian Dam proof white
* Brush and roller finishing
* 1x1 (Rate Rs.12)

1. All Walls (Quality: ACE):

* 1st Coat Apex (Rate Rs. 10)
* Final Coat Apex (Rate Rs. 9)

1. All Walls (Quality: APEX):

* 1st Coat Apex (Rate Rs. 13)
* Final Coat Apex (Rate Rs. 12)

1. Glass Cleaning Final Finishing:

* Water cleaning (free of cost)

1. Terrace Dam Proof:

* Washing from pressure water jet
* Crack filling 1 Coat
* Base white 1 Coat
* Terracotta/Gray 2 Coats
* 1x1 (Rate Rs. 40)

1. Parking Area:

* 2 Coats Enamel Yellow lines
* Lumpsum Amount (Rs. 30,000)
* INSIDE:

1. Walls:

* 1 Coat Asian crack filling
* 1 Coat touch up putty
* 1 Coat touch up dam proof
* Emery
* Removing fungus area apply waterproof putty 2 Coats
* Dam proof for fungus area
* Lumpsum Amount (Rs. 20,000)

1. Ceiling and Walls (Quality: Tractor Emulsion):

* 1st Coat Tractor Emulsion (Rate Rs. 7)
* Final Coat Tractor Emulsion (Rate Rs. 6)

1. Ceiling and Walls (Quality: Premium Emulsion):

* 1st Coat Premium Emulsion (Rate Rs. 10)
* Final Coat Premium Emulsion (Rate Rs. 9)

Note:

* Dam proof and walls 5years warranty
* Inspection is done for every year once
* Packing covers will be covered for all the floors before starting.
* The rates quoted shall be inclusive of all taxes, material, and labour.
* Quality of material shall be of good quality and as per requirements and Specifications mentioned.
* Asian paints will be used for all the material.
* Advance 50% on payment basis.

Yours’s faithfully

*(LOKESH.K)*